---------------------------------------------------------------------
File:      changelog.txt
Generated with Changelog Generator Version: 1.03r0
---------------------------------------------------------------------



Version: Current release                                                                  Revision: 5871      13.01.2014
========================================================================================================================
BUG:      Fixed problem while reading out apn settings in combination with PHS8 modem
CHG:      Add ysignald to taf startup / shutdown script
CHG:      Update external buildroot base linkage to v3_00r4
NEW:      add ysignald v1_00r0 to RFS


Version: v3_02r1                                                                          Revision: 5724      12.12.2013
========================================================================================================================
BUG:      Add gpsd start procedure to gps_start script instead to gps script.
          gpsd daemon locks the gps port now. At stop the daemon will be killed
BUG:      close all existing data connection before shut down the gsm modem.
CHG:      - Improve gsm start routine
          - Improve automatic gprs provider selection
CHG:      Update STW_YCOM_TOOLS to version v0_07r0
CHG:      - Update to toolchain version v1_20r0
          - Update to buildroot base version v3_00r1
CHG:      Update to
          ysysd v1_08r1
          yserverd v3_00r3
          ysmsd v1_06r0
          ylogd  v2_03r0
          ydatad  v3_00r1
          ynetworkd v2_04r0
          ymeetd v1_02r2
          
          wlan_driver v3_03r0
          
          flash_client v1_01r1
          can_recorder v1_03r0      
          ycom_tools v0_0r1
          ycom_canbridge v0_06r1
          yweb v1_02r3
          ycom v0_12r0
          ycom_sds v0_05r2
          stupidftpd v1_08r2
          can_utilz v1_01r1
          show_gps v1_03r0
          stw_eep v1_03r1
          stw_gsmMuxd v1_01r1
CHG:      Update to newest ysysd daemon version v1_08r2
CHG:      Update to new gsmmuxd v1_02r0
CHG:      Update to new show_gps version v1_03r1
CHG:      gdbserver is also build from buildroot now
CHG:      update config files (rc.conf, gps script) for GPS hadling  
CHG:      Update following packages:
          - ysysd v1_08r4
          - ygpsd v3_00r4
          - owl221a v3_04r0
CHG:      Update following packages:
          - ygpsd v3_00r5
CHG:      Edited the GSM and GPS scripts so that the TC3G modules are supported
CHG:      Update following packages:
          - show_gps  from v1_03r1 to v1_04r1
CHG:      changed bootup and shutdown order of gps in /etc/init.d/rc.conf
CHG:      replace the wlan_init and bt script call withing the rc.conf file with the new wlan_bt script
CHG:      Update bt start/stop scripts for TC3G support
CHG:      - Add PHS8 support t the gsm start/stop scripts
          - Only start the gsmMuxd daemon if the ysmsd daemon is used. If not use the nativ interface --> much faster than with the gsmMuxd
CHG:      remove power on/off procedoure for the GNS module . The GNS module doesn't have the gps_power pin anymore
CHG:      Replace the wlan_init script with the wlan_bt script. The wlan_bt script starts both interfaces
CHG:      Update wlan start/stop scripts for TC3G support
CHG:      - Update show_gps to version v1_04r3
          - Update ynetworkd to version v2_04r3
          - Update ydatad to version v3-00r2
          - Update ylogd to verison v2_03r3
          - Update ysmsd to version v1_06r1
          - Update ypgsd to version v3_00r8
          - Update ymeetd to version v1_02r3
          - Update yserverd to version v3_00r4
CHG:      Only set system time to hardware clock in case that ygpsd doesn't set the hwclock
CHG:      Update to new buildroot base project v3_00r2
CHG:      increase fwprintenv version to v1_00r1
CHG:      Update can_recorder to version v1_04r1
CHG:      Update yserverd to version v3_00r5
CHG:      Update to new wlan driver v3_04r1
CHG:      Update to new fwprintenv version v1_00r2
CHG:      - Update ydatad to version v3_00r3
          - Update ylogd to version v2_03r4
          - Update ymeetd to version v1_02r4
          - Update ynetworkd to version v2_04r4
          - Update yserverd to version v3_00r6
          - Update ysmsd to version v1_06r2
          - Update ysysd to version v1_08r5
CHG:      - Update ycom_canbridge to version v0_06r2
          - Update ycom_client to version v0_12r1
CHG:      Update external buildroot base linkage to v3_00r3
CHG:      Remove eeprom checksum fix in case that the chechsum is invalid.
CHG:      Update to new wlan driver version v3_04r2
CHG:      Add example for configuring a WLAN ADHOC network on a specified frequency
CHG:      - Set interface configuration for EES3 and PHS8 modem to raw data connection
          - Before starting a new data connection via ppp, close the old one
          --> Both changes increase connect/reconnect speed
NEW:      Add wpa configuration expamle for "Client mode --- OPEN + username and password authentification"
NEW:      Add stw_timeout script to the RFS 
NEW:      Add nano text editor
NEW:      Update ygpsd to version v3_01r0
NEW:      Add socat to tc3 bsp


Version: v3_00r4                                                                          Revision: 4421      13.05.2013
========================================================================================================================
BUG:      Fixed pap-secrets problem in case there is no user and password for the chosen provider available 
BUG:      SSH key generation at first time boot is now  "read only filesystem" save. 
BUG:      Fixed problem with static/uboot ip configuration
BUG:      Fixed naming convention problem Y_TC3-xxx --> TC3-xxx
BUG:      fixed wrong default root directory in /etc/passwd
BUG:      - Fixed ticket #329 --> USB connected device take a long time before coming up at startup process
BUG:      remove status and reload case from messagebus script
          add check if messagebus is locked if so remove lock after stoping the dbus
CHG:      Update to stupid_ftp version v1_08r1 
CHG:      Update rc.conf exports description.
CHG:      Update  owl221a  wlan driver version to v3_01r0 
CHG:      Set UBI volume Size to 35 MB, remove ext2 image
CHG:      Update process for setting the correct apn values. Following features were implemented:
          - Support for mnc with 3digits (necessary for USA)
          - own provider apns can be added to /mnt/dataflash/stw/modem/apns-conf.xml
          - add fall-back level in case that no valid apn was found in the regular and customer apns-conf.xml file. In that case the apn settings in /mnt/dataflash/stw/modem/apn-default.xml file chosen 
CHG:      Remount /etc/ppp to temporary filesystem 
CHG:      DBUS uuid will not be longer created at startup. The uuid will be generated at RFS creation via buildroot 
CHG:      Update CAN configuration mechanism to work with kernel v2.6 and kernel v3.x
CHG:      - Update ysysd daemon to version v1_07r2
          - Update ygpsd daemon to version v2_00r1
          - Update ymeetd daemon to version  v1_01r1
          - Update ycom tools to version v0_06r2
          - Update wlan driver owl221a to version v3_01r1
          - Increase max RFS volume size to 54 MB
CHG:      - Hostname script is now compatible with kernel 3.4 and 2.6.27,
          - Hostname script is now RO filesystem compatible 
CHG:      Update to newest ydatad daemon v3_00r0 
CHG:      Update to newest ysmsd daemon v1_05r0 
CHG:      Update to newest ymeetd daemon v1_02r0 
CHG:      Update to newest ylogd daemon v2_00r0 
CHG:      Update to newest ynetworkd daemon v2_03r1 
CHG:      Increase udhcpc wait time to 5 seconds (default 3) to fit new requirements 
CHG:      Implement new mechanism to read out serial number, type and variant of the device 
CHG:      Update udhcpc configuration: udhcpc will try to get an ip up to 5 times. Between the retries, the used gap is 4 seconds. 
CHG:      Update ylogd to newest version v2_00r1 
CHG:      Update can recorder to newest version v1_02r1 
CHG:      Update to newest beeper scripts version v1_01r0
CHG:      Update to newest yserverd version v2_08r1 
CHG:      Update to newest can recorder version v1_02r2 
CHG:      Update ynetworkd to newest version v2_03r4
          Update yserverd to newest version v2_08r2
          Update wlan driver to newest version v3_02r1
CHG:      update wlan driver module to version v3_02r2
CHG:      - Remove & after bluetoothd in bt script because the daemon start always daemonized by default 
          - add "hciconfig hci0 piscan" instead of "dbus system call" for activating the discoverability
CHG:      Change rfcomm listen to watch --> Service will be automatically restarted is the serial
          connection is disconnected
CHG:      Disable RX antenna diversity functionality
CHG:      Fix eeprom checksum in hostname script if possible
CHG:      Update owl221A wlan driver to version v3_02r3
NEW:      - Add GPSD package
          - ADD NTPDATE package
NEW:      Add default setting for stw_eep
NEW:      Add lrzsz package for send/receive files via serial interface 
NEW:      Edited the RFS to run the TC3G 3G-Modem and GPS/GLONASS module


Version: v2_02r0                                                                          Revision: 3138      11.07.2012
========================================================================================================================
CHG:      Update to buildroot tag v2_02r0 


